| Revision History | ADSP Interface for Linux Application Note - TDM Renderer/Capture - |
| --- | --- |

| Rev. | Date | Description | |
| --- | --- | --- | --- |
| Page | Summary |
| 1.00 | Jan. 29, 2018 | - | New Create |
| 1.01 | Jun. 28, 2018 | - | Style Modify |
| 1.02 | Oct. 29, 2018 | 28 | Remove value 32kHz in range of output sample rate |
| 2.00 | Dec. 25, 2018 | - | Official Release |
| 6 | Add note the reason OMX\_SetupTunnel, OMX\_TeardownTunnel and UseBuffer unavailable(×) of TDM |
| 12, 13, 18 | Remove OMX\_SetupTunnel, OMX\_TeardownTunnel, OMX\_UseBuffer function |
| 12 | Change details of “OMX\_ErrorIncorrectStateTransition” |
| 28, 30 | Update note |